Since there are still limitations regarding the lighting within FS9 there are still a few
compromises having to be made. The Decal lighting is a good way to overcome this but uses
a fair amount of polygons and texture mapping. All fuselage and tail lighting make full
use of the new Decal lighting method. However the inspection light splashes on the wings
and engines are conventional night mapped textures which are simply controlled by the
landing lights switch.

With the default panel\Posky763\Pkycondassign.xml gauge the inspection light is controlled
by the "L" lights command and not the "CTRL+L" landing lights command. So for this instance
the alpha channel for the wings and engines night textures should be black instead of white.

Alternatively the modified panel\Posky763\Pkycondassign.xml gauge allows for the inspection
light on the fuselage to be controlled by the "CTRL+L" landing lights command which is then
consistent for when the alpha channel for the wings and engines night textures are white.

[CF6-80A Engines]
Os767CF6-80A_L.bmp

[CF6-80C Engines]
Os767cf6-80_L.bmp
Os767cf6-80_Pylon_L.bmp

[JT9D Engines]
Os767JT9D_L.bmp

[PW4000 Engines]
Os767PW4000_L.bmp

[RB211 Engines]
OS767RB211G_L.bmp

[200/300 Wings]
OS767Wing_L_L.BMP
OS767Wing_R_L.BMP

[400 Wings]
OS764Wing_R_L.BMP
OS764Wing_R_T.BMP

Philip Foglar