Pilatus PC7 REFERENCE INFORMATION

For detailed instructions on how to fly this aircraft, see the Aircraft Handbook. For standard procedures, see the Checklists tab.

MAx T/O Weight -- 5952lb
Max Aerobatic Weight -- 4180lb
Empty Weight -- 3074lb



VFE - Maximum Flaps Extended Speed
           135 KIAS (0-40 degrees flaps)

Vle - MAx Ger Operating Speed
	   135 KIAS
           
      
VNE - Never Exceed Speed
           270 KIAS


VSO - Stalling Speed in the Landing Configuration
          (maximum weight; rearward c.g.)
          63 KIAS



VY  -  Best Rate-of-Climb Speed
          90 KIAS (sea level) --> ESTIMATED
          




NOTE:  For explanations of speeds used on this tab, see "V-speeds" in the Glossary section of Help.