GRUMMAN G-21A GOOSE PROCEDURES
For detailed instructions on how to fly this aircraft, see the Goose Aircraft Information articles in the Learning Center. For suggested speeds, see the Reference page of the Kneeboard. Note that most actions can also be performed using the mouse.

To... | Press...
Display/hide main panel | SHIFT+1
Display/hide radios | SHIFT+2
Display/hide GPS | SHIFT+3
Display/hide landing panel | SHIFT+4
Display/hide electrical panel | SHIFT+5
Display/hide overhead panel | SHIFT+6
Display/hide floor panel | SHIFT+7
Display/hide fuel selector | SHIFT+8
Display/hide trim | SHIFT+9

BEFORE STARTINGENGINE |
[ ] Brakes | TEST AND SET (press CTRL+PERIOD key)
[ ] Electrical Equipment, Autopilot | OFF
[ ] Avionics Master Switch | OFF
[ ] Fuel Selector Valve | BOTH
ENGINE START |
Press CTRL+E to initiate engine autostart sequence, or:
[ ] Right Throttle | OPEN 1/4 INCH (press F3 or F2 as necessary)
[ ] Right Mixture | RICH (press CTRL+SHIFT+F3 until fully in)
[ ] Right Propeller Area | CLEAR
[ ] Right Ignition Switch | BOTH
[ ] Auxiliary Fuel Pump Switch | ON
[ ] Starter Switch | RIGHT (release when engine starts) (press M+PLUS key to R, L, Both, Start)
[ ] Left Throttle | OPEN 1/4 INCH (press F3 or F2 as necessary)
[ ] Left Mixture | RICH (press CTRL+SHIFT+F3 until fully in)
[ ] Left Propeller Area | CLEAR
[ ] Left Ignition Switch | BOTH
[ ] Starter Switch | LEFT (release when engine starts) (press M+PLUS key to R, L, Both, Start)
Then: |
[ ] Oil Pressure | CHECK
[ ] Auxiliary Fuel Pump | OFF
[ ] Flashing Beacon and Nav Lights | ON as required
[ ] Avionics Master Switch | ON
BEFORE TAKEOFF |
[ ] Parking Brake | SET (hard surface) (press CTRL+PERIOD)
[ ] Flight Controls | FREE AND CORRECT
[ ] Flight Instruments | CHECK and SET
[ ] Fuel Quantity | CHECK
[ ] Mixture | RICH (press CTRL+SHIFT+F3 until fully in)
[ ] Fuel Selector Valve | RECHECK BOTH
[ ] Elevator Trim | SET for takeoff (Num Lock off, press Num Pad 1 or 7)
[ ] Right Throttle | 1200 RPM (water) 2000 RPM (land) (press F3 or F2 as necessary)
[ ] Magnetos | CHECK <100 RPM max drop on each (press M+MINUS, then press M+PLUS to L, R, L, Both)
[ ] Left Throttle | 1200 RPM (water) 2000 RPM (land) (press F3 or F2 as necessary)
[ ] Magnetos | CHECK <100 RPM max drop on each (press M+MINUS, then press M+PLUS to L, R, L, Both)
[ ] Suction Gauge | CHECK
[ ] Engine Instruments and Ammeter | CHECK
[ ] Throttles | 1000 RPM or less (press F2 or F3 as necessary)
[ ] Strobe Lights | AS DESIRED
[ ] Radios and Avionics | SET (press SHIFT+2 to display radio stack)
[ ] Autopilot | OFF
[ ] Wing Flaps | UP
[ ] Brakes | RELEASE (press PERIOD key)
TAKEOFF |
[ ] Wing Flaps | UP
[ ] Power | 36.5 in. Hg
[ ] Propellers | 2300 RPM
[ ] Mixture | RICH (LEAN above 3000 feet) (press CTRL+SHIFT+F3 or CTRL+SHIFT+F2 as necessary)
[ ] Elevator Control | ROTATE (at 75 MPH)
[ ] Landing Gear | UP (hard runway) (press G)
[ ] Wing Floats | UP (water runway) (press SHIFT+6 to display overhead panel)
EN ROUTE CLIMB |
[ ] Power | 33 in. Hg (press F2 or F3 as necessary)
[ ] Propellers | 2200 RPM (press CTRL+F2 or CTRL+F3 as necessary)
[ ] Mixture | RICH (LEAN above 3000 feet) (press CTRL+SHIFT+F3 or CTRL+SHIFT+F2 as necessary)
CRUISE |
[ ] Power | 27 in. Hg (press F2 or F3 as necessary)
[ ] Propellers | 1900 RPM (press CTRL+F2 or CTRL+F3 as necessary)
[ ] Elevator Trim | ADJUST (Num Lock off, press Num Pad 1 or 7 as necessary)
[ ] Mixture | LEAN (press CTRL+SHIFT+F2 or CTRL+SHIFT+F3 as necessary)
DESCENT |
[ ] Power | AS DESIRED (press F2 or F3 as necessary)
[ ] Mixture | ADJUST for smooth operation (press CTRL+SHIFT+F3 as necessary)
[ ] Fuel Selector Valve | BOTH
BEFORE LANDING |
[ ] Fuel Selector Valve | BOTH
[ ] Mixture | RICH (press CTRL+SHIFT+F3 as necessary)
[ ] Landing/Taxi Lights | ON
[ ] Autopilot | OFF (press SHIFT+2 to display radio stack)
[ ] Airspeed | 90 MPH (downwind)
LANDING |
[ ] Airspeed | 90 MPH
[ ] Landing Gear | DOWN (hard runway) UP (water runway) (press G)
[ ] Wing Floats | DOWN (water runway) (press SHIFT+6 to display overhead panel)
[ ] Wing Flaps | 30 (all water landings-60 degrees flaps)
[ ] Touchdown | MAIN WHEELS FIRST
[ ] Landing Roll | LOWER NOSE WHEEL GENTLY
[ ] Braking | MINIMUM REQUIRED (press PERIOD key)
AFTER LANDING |
[ ] Wing Flaps | UP (press F6 as necessary)
SECURING AIRPLANE |
[ ] Parking Brake | SET (press CTRL+PERIOD)
[ ] Electrical Equipment | OFF
[ ] Mixture | IDLE CUT OFF (press CTRL+SHIFT+F2 until fully out)
[ ] Ignition Switch | OFF (press M+MINUS key until Off)

NOTE: This aircraft's real-world checklists have been modified for use with Flight Simulator.