Integrated Simavionics group 1 (ISG1) ver 1.4 Update

ADDITIONS:
---------

1) Smiths style FMS (gaugexx=ISG1!SMITHS_FMS). Also included is a brown version
   of the FMS to more closely match the 747-400,757/767 colors (gaugexx=ISG1!SMITHS_FMS_BR).

2) Boeing 737-300/500 style Navigation Display (Gauge name: gaugexx=ISG1!HW_B737_ND), also included, is a brown
   version of the navigation display (gaugexx=ISG1!HW_B737_ND), and a no background version gaugexx=ISG1!HW_B737_ND_NB.

3) EFIS Control Panel for the Navigation Display (gaugexx=ISG1!HW_B737_ND), also included is a brown version
   of the EFIS control panel.

4) Server gauge (gaugexx=ISG1!Server) allows 3rd party gauges to read some of the FMS data.

5) New subfolder /Extras added.
              - Brown background bitmap for the Nav Display (for the _NB version).
              - filler faceplate gauges (df727isgplate2.gau,df727isgplate2.gau) Have hot areas on them to open popup windows etc (contributed by Nick S).

6) New isg.cfg file parameters added.

   -  DispETALocalTime=1    ,(displays eta times in FMS as local times (defalt is now UTC time)).
   -  Lnav1xAtTod=1         ,(sets sim rate to 1x when reached TOD point (if its greater than 1x))
   -  LnavSetEnRouteFreqs=1 ,(auto-tunes freqs when in VNAV mode)
   -  ArmPauseAtTod=1       ,(Arms the pause at TOD feature. when armed its status displays in the GNSXLS Nav page 4/4, 

7) New (AircraftId).cfg file parameters added.
   -  ApprFlapsMin          ,(Line 1 flaps value displayed in Smiths FMS Approach  page)
   -  ApprFlapsMid          ,(Line 2 flaps value displayed in Smiths FMS Approach  page)
   -  ApprFlapsMax          ,(Line 3 flaps value displayed in Smiths FMS Approach  page)
   -  ClbAltRest            ,(Default climb max Altitude for climb speed restriction)
   -  ClbSpdRest            ,(Default climb speed restriction displayed in Smiths FMS CLB page)
   -  ClimbIas=             ,(default climb Ias speed set in VNAV mode)
   -  CostIndex             ,(Default Cost Index value displayed in Smiths FMS perf page (range 0-200)
   -  CruiseIas=            ,(default cruise Ias speed set in VNAV mode)
   -  ClimbIasMin=          ,(Displays as Min climb speed in Smiths FMS perf limits page)
   -  ClimbIasMax=          ,(Displays as Max climb speed in Smiths FMS perf limits page)
   -  CruiseIasMin=         ,(Displays as Min cruise speed in Smiths FMS perf limits page)
   -  CruiseIasMax=         ,(Displays as Max cruise speed in Smiths FMS perf limits page)
   -  DescentIas=           ,(default descent Ias speed set in VNAV mode)
   -  DescentIasMin=        ,(Displays as Min cruise speed in Smiths FMS perf limits page)
   -  DescentIasMax=        ,(Displays as Max cruise speed in Smiths FMS perf limits page)
   -  DescAltRest           ,(Default descent max Altitude for climb speed restriction)
   -  DescSpdRest           ,(Default descent speed restriction displayed in Smiths FMS CLB page)
   -  EngThrust=(name)      ,(Displays as Engine thrust value in Smiths FMS)
   -  LdgFlaps=             ,(Default landing flaps value displayed in Smiths FMS approach page)
   -  LdgFlaps=             ,(Default landing flaps value displayed in Smiths FMS approach page)
   -  LnavSetEnRouteFreqs=1 ,(auto-tunes freqs when in VNAV mode)
   -  LnavOffAtLastWpt=1    ,(turns off LNAV on reached last LNAV waypoint;
   -  ModelId=(name)        ,(Displays as Aircraft model name in Smiths FMS)
   -  PerformanceData=(filename) , specifies aircraft performance data file to be loaded for FMS calculations.
   -  ToFlaps=              ,(Default takeoff flaps value displayed in Smiths FMS takeoff page)
   -  ToFlapsRange=         ,(Allowable FMS flaps entry values in Smiths FMS (comma delimited))
   -  V1=                   ,(Default V1 speed value displayed in Smiths FMS takeoff page)
   -  VR=                   ,(Default VR speed value displayed in Smiths FMS takeoff page)
   -  V2=                   ,(Default V2 speed value displayed in Smiths FMS takeoff page)
   -  VrefMin               ,(Line 1 Vref speed value displayed in Smiths FMS Approach  page)
   -  VrefMid               ,(Line 2 Vref speed value displayed in Smiths FMS Approach  page)
   -  VrefMax               ,(Line 3 Vref speed value displayed in Smiths FMS Approach  page)
   -  VnavOffAtLastWpt=1    ,(turns off VNAV on reached last LNAV waypoint;
   -  VnavOffOnManAltChg=1  ,(turns off VNAV if altitude is manually changed in the autopilot MCP)
   -  VnavSetSpd=0          ,(Does not set speed when VNAV is on (1 is default))
   -  VnavSetAlts=0         ,(when set to '0' VNAV will only set vertical speed. alitudes must be entered manually,(default is '1)).
   -  VnavSetSpdOffOnManSpdChg , turns off VNAV speed setting if manual speed change is detected while in VNAV mode.
   -  VnavSetSpdRestDist=   ,(sets the inbound distance from a speed restriction point, VNAV applies the restricted speed (default is 25 nm).
   -  WeightUnit=kgs        ,(Displays FMC weights in kgs (lbs default))


MODIFICATIONS:
------------------
EFS50_EHSI  -  Vertical deviation scale added (NAV/MAP modes) (displays only in descent when VNAV is on)
EFS50_EADI  -  LNAV, VNAV, and APR annunciators added.

FIXES:
--------------
EHSI          -  Glideslope indicator does not go all the way to the end of the scale (fixed)
EHSI          -  HSI mode - VOR2 indicator displayed incorrectly (fixed)
GNSXLS        -  CTD on startup if FSCommander created .pln file is in flightplans sub-folder. (Fixed)
GNSXLS        -  Fpl page - If fplan file list is 25 pages, when selecting 'NEW FPL', CTD occurs (Fixed)
GNSXLS        -  Awy page - CTD occurs when selecting an airway with more than 100 wpts (ex V16). (Fixed)
GNSXLS        -  Plan page - 1/6 , ETE mins display missing leading zero. (Fixed)
GNSXLS        -  App page - When app type is selected runway list is not filter to show only rwys avail for that app type. (fixed)
GNSXLS        -  NAV page 4 - current displayed longtiude value frozen at N74-22-44 (Fixed)
GNSXLS        -  Awy page - in some cases the awy page is set to '0' instead of one, which cases the airway data not to be displayed (Fixed).
MCU           -  VNAV annunciator overlaps HOLD annunciator when both modes are on. (Fixed)
MCU           -  Legs page , Dest cross alt read -999 when FP is modified in GNSXLS (see KDSM-KMDW route)


Requirements:
---------------------------------------
Windows XP / Vista
Microsoft Flight Simulator 2004 or Microsoft Flight Simulator X

Installation:
---------------------------------------
Run the Installer program and select your FS9 or FSX root folder for Install.

This will overwrite and update your existing ISG files.

Limitations:
---------------------------------------
This is an update Install only, not a full install.  ISG1 will not work properly unless the
full Installer is already installed on your machine prior to installing this update.

Regards.
Ernie Alston ISG1 Developer.

Email  alstoer1@compuserve.com
AIM:   alstoer1
Website  http://isgsim.com
