POSKY CRJ-200 CHECKLIST AND PROCEDURES
<Note:> Not to be used for real-world navigation.
For detailed instructions on how to fly this aircraft, see the Aircraft Handbook. For suggested speeds, see the Reference tab.

____________________________________
BEFORE ENGINE START

PARKING BRAKE				SET
ENSURE BRAKES ARE SET

FUEL QUANTITY/BALANCE			CHECKED
CHECK THAT FUEL MEETS AMOUNT REQUIRED FOR FLIGHT AND IS BALANCED PROPERLY

CABIN SIGNS				SET
SEATBELT SIGN AND NO SMOKING SIGNS 	ON

FLIGHT INSTRUMENTS/BUGS			SET
CHECK FOR PROPER ALTIMETER SETTING,
NO FAILURE FLAGS AND AIRSPEED BUGGED FOR PROPER TAKEOFF V-SPEEDS. ALTITUDE ALERT SET FOR DEPARTURE CLEARANCE
NAV RADIOS/FMS				SET
RADIOS ARE SET UP FOR DEPARTURE ROUTE AND PROPER FLIGHT PLAN/DEPARTURE ENTERED INTO FMS

BLEEDS/AIRCONDITIONING			SET
ENGINE/APU BLEEDS OPEN AND AIR COND. PACKS SHUT OFF FOR ENGINE START

EXTERIOR LIGHTS				SET
NAV LIGHTS ON, BEACON LIGHTS ON

____________________________________
AFTER START

Press CTRL+E to initiate engine autostart sequence, or:
 
PITOT HEAT		ON
PITOT HEAT CHECKED 	ON
WINDOW HEAT		ON
WINDOW HEAT CHECKED 	ON

ANTI-ICE		AS REQ
SELECT ENGINE ON IF ICING CONDITIONS EXIST

BLEEDS/AIRCONDITIONING	SET
ENGINE BLEEDS OPEN, APU BLEED CLOSE AIRCONDITIONING PACKS ON AND ON ENGINE BLEEDS

ELECTICAL PANEL		SET
ELECTRICAL PANEL SET TO GENERATORS

APU	OFF
AFTER 2 MINUTE COOL DOWN PERIOD SELECT APU OFF

____________________________________
TAXI AND BEFORE TAKEOFF

CABIN CREW	NOTIFIED
ON CYCLE OF NO SMOKING SIGN(2 CHIMES)

TRANSPONDER	ON
ENSURE TRANSPONDER IS ON AND PROPER CODE IS SET

BLEEDS/AIRCONDITIONING	SET
SELECT AIR CONDITIONING PACKS TO PROPER SETTING BASED ON TAKEOFF PERFORMANCE

EXTERIOR LIGHTS	ON
LANDING LIGHTS AND STROBE LIGHTS ON

PARKING BRAKE	OFF
ENSURE PARKING BRAKE IS RELEASED

BRAKES			CHECKED
SOFTLY TEST BRAKES

FLAPS/SLATS		SET
ENSURE FLAPS AND SLATS ARE SET AT PROPER TAKEOFF SETTING

FLIGHT CONTROLS		CHECKED
COMPLETE FULL LEFT/RIGHT AILERON CHECK, FULL TRAVEL ELEVATOR CHECK AND FULL LEFT/RIGHT RUDDER DEFLECTION

TAKEOFF BRIEFING	COMPLETE
BRIEF ON FOLLOWING ITEMS:
TAKEOFF TYPE- ROLLING OR STATIC
TAKEOFF RUNWAY
ABORT CONSIDERATIONS
AIRBORNE EMERGENCY CONSIDERATIONS AND
RETURN TO FIELD CONSIDERATIONS
V-SPEEDS
DEPARTURE PROCEDURE/ROUTE NAV RADIOS AND TRANSPONDER CODE ALTITUDE LIMIT
ANTI-ICE AND WEATHER FACTORS

____________________________________
RUNWAY LINEUP

[ ] Lights -- ON

____________________________________
TAKEOFF

[ ] Thrust Lever -- T/O
     (press F3 until T/O)
[ ] Brakes -- RELEASE
     (press PERIOD key)
[ ] VR -- ROTATE

____________________________________
AFTER TAKEOFF

LANDING GEAR	UP/LTS OUT
ENSURE LANDING GEAR IS RETRACTED AND IN TRANSIT LIGHTS ARE OUT

CLIMB POWER	SET
SET CLIMB POWER

FLAPS/SLATS	UP
AFTER MINIMUM SPEEDS, ENSURE FLAPS AND SLATS ARE RETRACTED

BLEEDS/AIRCONDITIONING	SET
ENSURE AIRCONDITIONING PACKS ARE ON

ANTI-ICE	AS REQD
ENSURE ENGINE AND WING ANTI-ICE ON IF ICING CONDITIONS ARE PRESENT

ABOVE 10,000FT:

LANDING LIGHTS	OFF


____________________________________
CLIMB
ABOVE 18,000FT:
ALTIMETERS	RESET
RESET ALTIMETERS TO 29.92

____________________________________
CRUISE

CRUISE POWER	SET
SET POWER TO CRUISE SETTING

CABIN SIGNS	AS REQD
SEATBELT SIGN AT CAPTAINS DISCRETION


____________________________________
DESCENT

CABIN SIGNS	ON
SEATBELT AND NO SMOKING SIGNS ON

ANTI-ICE	AS REQD
SELECT ENGINE AND WING ANTI-ICE ON IF ICING CONDITIONS ARE PRESENT OR WILL BE ENCOUNTERED

FLIGHT INSTRUMENTS/BUGS	SET
SET AIRSPEED BUG TO LANDING VREF CHECK ALTIMETERS ARE SET TO LANDING ATIMETER SETTING

NAV RADIOS/FMS	SET
SET RADIOS FOR LANDING RUNWAY OR APPROACH. SET ARRIVAL PROCEDURE AND APPROACH IN FMS

APPROACH BRIEFING	COMPLETE

APPROACH BRIEFING SHOULD INCLUDE:
APPROACH TYPE AND LANDING RUNWAY
FREQUENCIES
FINAL APPROACH COURSE
MINIMUM ALTITUDES
VREF SPEEDS
MISSED APPROACH PROCEDURES ANY SPECIAL CONSIDERATIONS-ICE/WET RUNWAY ETC...

___________________________________
BEFORE LANDING

CABIN CREW	NOTIFY
ONE CYCLE OF NO SMOKING SIGN(2 CHIMES)

LANDING GEAR	DOWN/GREEN
CHECK LANDING GEAR IS EXTENDED AND ALL GREEN LIGHTS ARE ILLUMINATED WITH NO RED/UNSAFE LIGHTS SHOWING

FLAPS/SLATS	SET
CHECK LANDING FLAPS ARE SET IN FINAL LANDING CONFIGURATION

SPEEDBRAKES	ARM
ENSURE SPEEDBRAKES ARE ARMED FOR AUTODEPLOY

AUTOBRAKES	SET
IF NEEDED, SET AUTOBRAKES TO PROPER SETTING FOR RUNWAY CONDITION/LENGTH
____________________________________
LANDING

[ ] Brakes -- AS REQUIRED
     (press PERIOD key)
[ ] Spoilers -- VERIFY EXTENDED

____________________________________
AFTER LANDING/CLEARING RUNWAY

EXTERIOR LIGHTS	SET

LANDING LIGHTS, WING AND STROBE LIGHTS OFF
PITOT HEAT	OFF

WINDOW HEAT	OFF

ANTI-ICE	AS REQD
WING HEAT OFF, ENGINE ANTI-ICE ON IF ICING CONDITIONS ARE PRESENT
FLAPS		UP
RETRACT FLAPS/SLATS

SPEEDBRAKES	RETRACTED
RETRACT AND STOW SPEEDBRAKES

TRANSPONDER	STBY
PLACE TRANSPONDER TO STANDBY
APU	START
START APU FOR GROUND USE

BLEEDS/AIRCONDITIONING	SET
BLEEDS AND PACKS CONFIGURED FOR GROUND USE


____________________________________
SHUTDOWN

PARKING BRAKE	SET
SET PARKING BRAKES

ELECTRICAL PANEL	SET
SET ELECTRICAL PANEL TO APU OR GROUND POWER

BLEEDS/AIRCONDITIONING	SET
SET PACKS TO APU/EXTERNAL AIR AND CLOSE ENGINE BLEEDS

ANTI-ICE	OFF
CLOSE ENGINE ANTI-ICE VALVES

START LEVERS	CUTOFF
PLACE ALL START LEVERS TO CUTOFF AND WATCH FOR INDICATIONS OF ENGINE SHUTDOWN

CABIN SIGNS	SET
SEAT BELT SIGN OFF

EXTERIOR LIGHTS	SET
BEACON AND TAXI LIGHTS OFF, NAV LIGHTS ON



NOTE: This aircraft's real-world checklists have been modified for use with Flight Simulator 2002. To learn about using, printing, and customizing checklists, see Help.