Mirage's FMS-6000 gauge.
Version 0.1 Alpha Step58

Copyright (c)2006 Yasutoshi Mori.
All Rights Reserved.

http://mirage.orz.ne.jp/fsdev/
Opteron150@hotmail.com


Description
===========

This is FMS gauge for FS2004.
This gauge modeled Rockwell Collins's FMS-6000.



Requirement
===========

*MSFS 2004
*FSUIPC( Note1)
*AIRAC for PMDG( Note2 )
*GDI+

Note1:Registered version is necessary.
Note2:AIRAC can be downloaded from NavData( http://www.navdata.at/ )



Installation
============

1:Extract All files and copy it onto the FS2004's gauges folder.

2.Edit panel.cfg.
Example:
gaugexx=MIR_FMS!FMS6000, 0, 0, 500, 559
gaugexx=MIR_FMS!AP85, 0, 0, 500, 158

3.AIRAC is required, to use NAV/FIX and Airway data.
Download AIRAC data from NavData site and install it.


Working function
================

A part of FPL page
Airlane reading
A part of LEGS page
A part of INDEX page
A part of STATUS page
NAVFIX\NAVRAD data reading
LNAV tracking
VNAV(temporary)



Function under development
==========================

SID/STAR data reading
speed constrain
BELOW and ABOVE of Alt constrain of LEGS
scratch pad Behavior
STATUS page
SID/STAR page
PERF page
VNAV-PATH Behavior
FORECAST at DESCEND
COROUTE reading and writing
sphere route calculation when long distance flies
COROUTE
setting file for each aircraft



Limitation in specification
===========================

At present, FMS control the value of HDG, ALT, and VS.



Known problem
=============

-FMS is reset when resizing it. 
-CTD sometime.


Configuration file
==================

FMSSt6000.lua is configuration file.
You can edit weight, climb and descend value.
Default value is set for FS2004's LeaJet45.




Exemption matters
=================

*This gauge is Alpha test.
*The author doesn't take the responsibility for any accident or data damage, etc. that occur because of the use of this gauge.
