##
8-0 Fuel System ECAM Display

1.
A green vertical bar indicates that the Engine feed valve is open. An orange horizontal bar indicates that the valve is closed.
2.
A green vertical bar indicates that the APU feed valve is open. An orange horizontal bar indicates that the valve is closed.
3.
The green squares with a vertical line in them indicate that the outer tank pumps are on. A green square with a horizontal line indicates that the pump have been turned off by the fuel system logic. An orange square with a horizontal line indicates that the fuel pumps have been switched off by the pilot.
The green number below the fuel pump indicators is the fuel quantity for the corresponding tank.
4.
Same as 3. just for the inner tanks.
5.
Same as 3. just for the center tank.
6.
Indication of total fuel on board.