Tu-154B-2 REFERENCE INFORMATION

Total Flight Simulator aircraft weight with full fuel
           98000 kG.

NOTE: To adjust fuel load, on the Aircraft menu, click Fuel.

VMO - Maximum Operating Speed (airspeed)
           650 IAS, km/h

MMO - Maximum Operating Speed (Mach)
            .88 Mach

VLO - Maximum Gear Operating Speed
           330 IAS, km/h

VLE - Maximum Landing Gear Extension Speed
           400 IAS, km/h

Maximum Flap (Placard) Speeds
        Flaps 15	420 IAS, km/h
	Flaps 28	360 IAS, km/h
	Flaps 45	300 IAS, km/h

V1 - Takeoff Decision Speed(dry runway, flaps 28)
        Standard temperature, sea level pressure altitude
              240 IAS, km/h (98000 kG.)
        Standard temperature, 1000m pressure altitude
              245 IAS, km/h (98000 kG.)        
        
VR - Rotation Speed (dry runway, flaps 28)
        Standard temperature, sea level pressure altitude
              270 IAS, km/h (98000 kG.)
        
V2 - Takeoff Safety Speed (dry runway)
        Standard temperature, sea level pressure altitude, flaps 28
              280 IAS, km/h (98000 kG.)
        Standard temperature, sea level pressure altitude, flaps 15
              296 IAS, km/h (98000 kG.)
        Standard temperature, sea level pressure altitude, flaps 0
              365 IAS, km/h (98000 kG.)

VREF - Landing Approach Speed (flaps 45, gear down)
             275 IAS, km/h (80000 kG.)
