Tu-154B-2 PROCEDURES

For detailed instructions on how to fly this aircraft, see the Aircraft Handbook. For suggested speeds, see the Reference tab.

____________________________________
PUSHBACK (if parked at a gate)
[ ] Request Pushback -- SET
     (press SHIFT+P key)

____________________________________
BEFORE START

[ ] Parking Brake -- SET
     (press CTRL+PERIOD key)
[ ] Nav Light Switch -- ON

____________________________________
ENGINE START

[ ] Battery Switch -- ON
[ ] Fuel Tanks Selector -- AUTOMAT ON
[ ] Engine Start 2 -- ON
[ ] Fuel 2 -- ON
[ ] Generator 2 -- ON
[ ] Engine Start 1 -- ON
[ ] Fuel 1 -- ON
[ ] Generator 1 -- ON
[ ] Engine Start 3 -- ON
[ ] Fuel 3 -- ON
[ ] Generator 3 -- ON

____________________________________
AFTER START

[ ] Flight Controls -- CHECK
[ ] Autopilot -- SET AND OFF
[ ] Battery Switch -- OFF
[ ] Instruments -- CHECKED
[ ] Avionics Switch -- ON
[ ] Avionics -- SET
[ ] Trim -- SET


____________________________________
BEFORE TAKEOFF

[ ] Beacon Light Switch -- ON

____________________________________
ON TAXI-WAY

[ ] Transponder -- ALT
     (press SHIFT+2 to display radio stack)
[ ] Thrust Levers -- ADVANCE TO 75-80%
    (press F2 or F3 as necessary)
[ ] Altimeter -- SET TO 0 M
[ ] Flaps -- SET FOR TAKEOFF
     (press F7 Two times, 28 deg)
[ ] Spoilers -- OFF
     (press / )
[ ] Pitot -- AS REQUIRED


____________________________________
ON A RUNWAY

[ ] Brakes -- RELEASE
     (press PERIOD key)
[ ] Thrust Levers -- ADVANCE SMOOTHLY TO 100% N1
    (press F2 or F3 as necessary)
[ ] Landing Lights -- ON
[ ] Brakes -- off
[ ] Airspeed 180 km/h-- CALLOUT "180"
[ ] Airspeed V1 -- CALLOUT "V1"
[ ] Airspeed VR -- CALLOUT "ROTATE"
                           -- ROTATE TO APPROX. 6-8 DEGREES PITCH UP
[ ] Airspeed V2 -- CALLOUT "V2"
[ ] Landing Gear -- UP (WHEN POSITIVE CLIMB ESTABLISHED)
     (press G)
[ ] Airspeed --MAINTAIN V2+30 km/h
[ ] Flaps-- START RETRACT AT 120 M
    (press F6 as necessary)

____________________________________
CLIMB

[ ] Autopilot -- ENGAGE
[ ] Autothrottle -- OFF
[ ] Landing Lights -- OFF
[ ] Altimeter -- SET TO 29.92 CROSSING 900 M

____________________________________
CRUISE

[ ] Thrust Levers-- AS DESIRED
    (press F2 or F3 as necessary)
[ ] Trim -- AS NECESSARY
     (press Num Pad 6 or Num Pad 7 as necessary)

____________________________________
DESCENT

[ ] Airspeeds (VREF, VAPP) -- COMPUTED AND SET
     (see the Reference tab of the Kneeboard)
[ ] Pitot -- AS REQUIRED
[ ] Autopilot -- AS DESIRED
[ ] Airspeed -- 500 km/h BELOW 3000 M
[ ] Thrust Levers -- AS DESIRED
    (press F2 or F3 as necessary)
[ ] Avionics -- SET
[ ] Altimeter -- SET TO LOCAL SETTING CROSSING TRANS LEVEL
[ ] Approach Procedure -- REVIEW

____________________________________
APPROACH

[ ] Autopilot -- AS DESIRED
[ ] Airspeed -- 400 km/h
[ ] Landing Gear -- DOWN and CONFIRMED
     (press G)
[ ] Flaps -- 15 deg
     (press F7 )
[ ] Airspeed -- 350 km/h
[ ] Flaps -- 28 deg
     (press F7 )
[ ] Airspeed -- 300 km/h


____________________________________
LANDING

[ ] Flaps -- 45 deg
     (press F7 )
[ ] Thrust Levers -- AS DESIRED
    (press F2 or F3 as necessary)
[ ] Landing Lights -- ON BELOW 600 M
[ ] Airspeed -- 275 km/h
[ ] Autopilot -- OFF
[ ] Autothrottle -- OFF
[ ] AutospoIler -- SET


____________________________________
LANDING ROLL

[ ] Thrust Levers - CLOSED
    (press F1 at Alt no more 4-5 M)
[ ] Thrust Levers-- REVERSE
     (press F2 until Reverse)
[ ] Thrust Levers -- IDLE AT 120 km/h
     (press F3 until Idle)
[ ] Brake -- AS NECESSARY
     (press PERIOD key)

____________________________________
TAXI-IN

[ ] Lights -- AS DESIRED
[ ] Flap Lever -- UP
     (press F5 )
[ ] Transponder -- STBY
[ ] Pitot -- OFF
[ ] Spoilers -- OFF
     (press / )
[ ] Engine Start 2 -- OFF
[ ] Generator 2 -- OFF


____________________________________
PARKING

[ ] Parking Brake -- SET
     (press CTRL+PERIOD KEY)
[ ] Avionics Switch -- OFF
[ ] Generator 1,3 -- OFF
[ ] Engine Start 1,3 -- OFF
[ ] Fuel Tanks Selector -- CUTOFF




