ALPHA MiG-25 Foxbat REFERENCE INFORMATION

For standard procedures, see the Checklists tab.

Total Flight Simulator aircraft weight with full fuel
           90,585 lbs

NOTE: To adjust fuel load, on the Aircraft menu, click Fuel.

VSO - Stalling speed, clean
	179 KIAS (90,585 lbs)

VMO - Maximum Operating Speed (airspeed)
           1200 KIAS (primary display)

MMO - Maximum Operating Speed (Mach)
            2.82 Mach


VA  -  Maneuvering Speed
          90,585 lbs.
                    250 KIAS (sea level)
                    325 KIAS (20,000')
                    400 KIAS (40,000')

VLO - Maximum Gear Operating Speed
           350 KIAS

VLE - Maximum Landing Gear Extension Speed
           400 KIAS

VFE - Maximum Flaps Extended Speed
          300 KIAS (flaps 10 degrees)
          270 KIAS (flaps 20 degrees)
          240 KIAS (flaps 30 degrees)
          225 KIAS (flaps 40 degrees)

V1 - Takeoff Decision Speed (dry runway; standard temperature)
       160 KIAS (for all conditions, with anti-skid off)

VR - Rotation Speed (dry runway; standard temperature)
        Sea Level
                   200 KIAS (90,585 lbs)

        5,000'
                   200 KIAS (90,585 lbs)


V2 - Takeoff Safety Speed (dry runway, standard temperature)
        Sea Level
                  225 KIAS (90,585 lbs)

        5,000'
                   170 KIAS (90,585 lbs)


VAPP - Approach Climb Speed (1/2 flaps; gear up)
             <4,000'
                  225 KIAS (67,162 lbs)

             5,000'
                   225 KIAS (67,162 lbs)


VREF - Landing Approach Speed (full flaps; gear down)
             <4,000'
                  225 KIAS (67,162 lbs)

             5,000'
                   225 KIAS (67,162 lbs)


Best Glide Speed
           225 KIAS (gear and flaps up; both engines inoperative)


NOTE:  For explanations of speeds used on this tab, see "V-speeds" in the Glossary section of Help.