Prototype TU-144 Aircraft 00-1 (CCCP-68001)
-------------------------------------------
Overall Length 					194' 9" - 59.40 m
Height from ground (ground to top of fin) 	40' 2" - 12.25 m
Height from lowest point (Engine) 		34' 5" - 10.50 m
Fuselage max external Width 			11' 5" - 3.50 m
Fuselage max external Height 			10' 7" - 3.25 m
Wing Span 					90' 7" - 27.65 m
Wing Length (Root Chord) 			111' 3" - 33.90 m
Wing Area 					4,715' ft² - 438 m²
Main Gear Track 				30' 2" - 9.20 m

Pre-Production TU-144S Aircraft 01-1 (CCCP-77101)
------------------------------------------------
Overall Length 					215' 6" - 65.70 m
Wing Span 					91' 9" - 28 m
Wing Length (Root Chord) 			99' 4" - 30.30 m
Wing Area 					5,414 ft² - 503 m²

Production TU-144S, TU-144D and TU-144LL
----------------------------------------
Overall Length 					215' 6" - 65.70 m
Height from ground (ground to top of fin) 	47' 3" - 14.40 m
Height from lowest point (Engine) 		42' 2" - 12.85 m
Fuselage max external Width 			11' 3" - 3.45 m
Fuselage max external Height 			11' 5" - 3.50 m
Wing Span 					94' 6" - 28.80 m
Wing Length (Root Chord) 			104' 7" - 31.90 m
Wing Area 					5,457 ft² - 507 m²
Main Gear Track 				19' 1" - 5.80 m

Speeds and Distances
-------------------
Maximum Speed 	
TU-144 		1,510 mph - 2,430 km/h (M 2.30)
TU-144S 	1,550 mph - 2,500 km/h (M 2.35)
TU-144D 	1,420 mph - 2,285 km/h (M 2.15)
TU-144LL 	1,550 mph - 2,500 km/h (M 2.35)

Cruising Speed 	
TU-144 		1,430 mph - 2,300 km/h (M 2.17)
TU-144S 	1,365 mph - 2,200 km/h (M 2.07)
TU-144D 	1,315 mph - 2,120 km/h (M 2.00)
TU-144LL 	1,430 mph - 2,300 km/h (M 2.17)

Maximum Permissible Range 	
TU-144 			1,815 ml - 2,920 km
TU-144S Subsonic 	2,672 ml - 4,300 km
	7 tons 		2,237 ml - 3,600 km
	15 tons 	1,914 ml - 3,080 km
TU-144D 7 tons 		3,853 ml - 6,200 km
	11 tons 	3,542 ml - 5,700 km
	13 tons 	3,418 ml - 5,500 km
	15 tons 	3,312 ml - 5,330 km
TU-144LL 		2,485 ml - 4,000 km

Take-off Speed 					220 mph - 355 km/h
Landing Approach Speed 				180 mph - 290 km/h
Landing Speed 					168 mph - 270 km/h
Maximum Landing Gear Speed 			283 mph - 455 km/h
Maximum Nose Down (17 degrees) Speed 		283 mph - 455 km/h
Maximum Forward Cannards Deployed Speed 	280 mph - 450 km/h
Maximum Operating Altitude 			65,500 ft - 20,000 m
Take-off Runway Length 				9,613 ft - 2,930 m
Landing Runway Length 				8,432 ft - 2,570 m

Weights
Prototype TU-144 (Kuznetsov NK-144 engines)
Max Weight Without Fuel 	187,400 lbs - 85,000 kg
Max Take Off Weight 		396,800 lbs - 180,000 kg
Max Weight of Fuel 		154,300 lbs - 70,000 kg

TU-144S (Kuznetsov NK-144A engines)
Max Weight Without Fuel 	202,400 lbs - 91,800 kg
Max Payload 			33,000 lbs - 15,000 kg
Max Take Off Weight 		429,900 lbs - 195,000 kg
Max Landing Weight 		264,500 lbs - 120,000 kg
Max Weight of Fuel 		216,000 lbs - 98,000 kg

TU-144D (Koliesov RD-36-51A engines)
Max Weight Without Fuel 	218,700 lbs - 99,200 kg
Max Payload 			33,000 lbs - 15,000 kg
Max Take Off Weight 		456,300 lbs - 207,000 kg

TU-144LL (Kuznetsov NK-321 engines)
Max Weight Without Fuel 	227,000 lbs - 103,000 kg
Max Take Off Weight 		447,500 lbs - 203,000 kg
Max Landing Weight 		275,500 lbs - 125,000 kg
Max Weight of Fuel 		209,440 lbs - 95,000 kg
