xplane_certified=v7.61
author=PRO Edition Team
author_web=http://www.x-plane.ch
release=v7
release_date=18-Sep-2004
plane_constructor=Airbus
plane_type=Heavy
plane_full_name=Airbus A330-223
plane_compagny=Qatar Airways
max_seats=293
cruise_altitude=41000
cruise_speed=480
climb_rate=1800
climb_speed=350
descent_rate=1800
descent_speed=350
maximum_range=6450
fuel_max_onboard=36786
fuel_max_consumption_hour=1590
###
# Added for CP
takeoff_flaps=2
takeoff_flaps_heavy=4
takeoff_flaps_heavy_threshold=450000
landing_flaps=6
###
# Optional equipment
HasRadarAltimeter=TRUE
# 0=none, 1=FMS/GPS, 2=Basic
AutoPilotType=1
###
# Text checklist items
# Separate the left hand and right hand text with a ':' and do
# not add extra space before/after ':'
CL_B4Start=Pressurization:Manual
CL_B4Start=Hydraulics:Set
CL_B4GateDeparture=Sliding Windows:Both Locked
CL_B4GateDeparture=Doors and slides:Green, Armed
CL_B4GateDeparture=Notify Swiss dispatcher:CHECK
CL_B4Taxi=ECAM Status:Checked
CL_Takeoff=Thrust Mode:Take Off
CL_Climb=Packs:On
CL_Climb=Engine Mode Selector:Normal
###
#
# Set V1, Vr and V2 for all possible flap settings (detents)
# Set the minimum and maximum airspeeds which are automatically
# mapped to the empty and max weights of the airplane
# Index is the flap detent, value is the KIAS
# Not all of the flap detents really make sense for takeoff
# but we can't anticipate all conditions so they should all
# be here.  You can have many [...]
V1Min[0]=130
V1Max[0]=90
V1Min[1]=130
V1Max[1]=90
V1Min[2]=130
V1Max[2]=90
V1Min[3]=130
V1Max[3]=90
V1Min[4]=130
V1Max[4]=90
V1Min[5]=135
V1Max[5]=92
V1Min[6]=138
V1Max[6]=93
VrMin[0]=135
VrMax[0]=172
VrMin[1]=130
VrMax[1]=161
VrMin[2]=121
VrMax[2]=151
VrMin[3]=115
VrMax[3]=144
VrMin[4]=109
VrMax[4]=137
VrMin[5]=102
VrMax[5]=127
VrMin[6]=113
VrMax[6]=126
V2Min[0]=155
V2Max[0]=205
V2Min[1]=150
V2Max[1]=190
V2Min[2]=139
V2Max[2]=175
V2Min[3]=132
V2Max[3]=166
V2Min[4]=125
V2Max[4]=158
V2Min[5]=115
V2Max[5]=145
V2Min[6]=115
V2Max[6]=142
# ------------------------------------------------
# Speed Climb (VVI and Speed)
# ------------------------------------------------
# VVI and speed are automatically set by CoPilot by Levels/Steps. (Note
the
# [1] is AGL, the other are Feets). You can have many [...]
speedclimbaltbottom[0]=0
speedclimbaltup[0]=1500
speedclimbspeedvvi[0]=3000
speedclimbspeed[0]=180
speedclimbaltbottom[1]=1500
speedclimbaltup[1]=5000
speedclimbspeedvvi[1]=3000
speedclimbspeed[1]=210
speedclimbaltbottom[2]=5000
speedclimbaltup[2]=10000
speedclimbspeedvvi[2]=3500
speedclimbspeed[2]=250
speedclimbaltbottom[3]=10000
speedclimbaltup[3]=15000
speedclimbspeedvvi[3]=3200
speedclimbspeed[3]=300
speedclimbaltbottom[4]=15000
speedclimbaltup[4]=20000
speedclimbspeedvvi[4]=2600
speedclimbspeed[4]=300
speedclimbaltbottom[5]=20000
speedclimbaltup[5]=25000
speedclimbspeedvvi[5]=2100
speedclimbspeed[5]=300
speedclimbaltbottom[6]=25000
speedclimbaltup[6]=30000
speedclimbspeedvvi[6]=2100
speedclimbspeed[6]=280
speedclimbaltbottom[7]=30000
speedclimbaltup[7]=35000
speedclimbspeedvvi[7]=1500
speedclimbspeed[7]=253
speedclimbaltbottom[8]=35000
speedclimbaltup[8]=38000
speedclimbspeedvvi[8]=1000
speedclimbspeed[8]=240
speedclimbaltbottom[9]=38000
speedclimbaltup[9]=40000
speedclimbspeedvvi[9]=1000
speedclimbspeed[9]=235
speedclimbaltbottom[10]=40000
speedclimbaltup[10]=41000
speedclimbspeedvvi[10]=900
speedclimbspeed[10]=230
# ------------------------------------------------
# Speed Descent (VVI and Speed)
# ------------------------------------------------
# VVI and speed are automatically set by CoPilot by Levels/Steps. (Note
the
# [1] is AGL, the other are Feets). You can have many [...]
speeddescentaltbottom[0]=0
speeddescentaltup[0]=3000
speeddescentspeedvvi[0]=650
speeddescentspeed[0]=133
speeddescentaltbottom[1]=3000
speeddescentaltup[1]=5000
speeddescentspeedvvi[1]=1000
speeddescentspeed[1]=180
speeddescentaltbottom[2]=5000
speeddescentaltup[2]=10000
speeddescentspeedvvi[2]=1100
speeddescentspeed[2]=230
speeddescentaltbottom[3]=10000
speeddescentaltup[3]=13000
speeddescentspeedvvi[3]=1200
speeddescentspeed[3]=250
speeddescentaltbottom[4]=13000
speeddescentaltup[4]=15000
speeddescentspeedvvi[4]=1500
speeddescentspeed[4]=270
speeddescentaltbottom[5]=15000
speeddescentaltup[5]=20000 
speeddescentspeedvvi[5]=1800
speeddescentspeed[5]=280
speeddescentaltbottom[6]=20000
speeddescentaltup[6]=30000 
speeddescentspeedvvi[6]=2300
speeddescentspeed[6]=300
speeddescentaltbottom[7]=30000
speeddescentaltup[7]=35000 
speeddescentspeedvvi[7]=3200
speeddescentspeed[7]=260
speeddescentaltbottom[8]=35000
speeddescentaltup[8]=41000 
speeddescentspeedvvi[8]=2900
speeddescentspeed[8]=230