#GoodWay v2.3.0
#Tue Sep 02 19:47:53 CEST 2003
cruise_speed=484
descent_rate=2000
descent_speed=290
plane_constructor=Boeing
xplane_certified=930b10
author=Reuben Horsley and the X-Plane Freeware Project
cruise_altitude=45000
plane_type=747-400
max_seats=524
plane_full_name=B747-400 Air Canada
release_date=Sun Jan 4 00:00:00 CET 2006
fuel_max_onboard=53248
climb_speed=340
plane_company=Air Canada
release=930
fuel_max_consumption_hour=4200
author_web=http\://www.x-plane.com
maximum_range=7392
climb_rate=2000
###
# Added for CP
takeoff_flaps=3
takeoff_flaps_heavy=3
takeoff_flaps_heavy_threshold=680000
landing_flaps=6
###
# Optional equipment
HasRadarAltimeter=TRUE
# 0=none, 1=FMS/GPS, 2=Basic
AutoPilotType=1
###
# Text checklist items
# Separate the left hand and right hand text with a ':' and do
# not add extra space before/after ':'
CL_B4Start=Pressurization:Auto
CL_B4Start=Hydraulics:Set
CL_B4GateDeparture=Sliding Windows:Both Locked
CL_B4GateDeparture=Doors and slides:Green, Armed
CL_B4GateDeparture=Notify dispatch:CHECK
CL_B4Taxi=ECAM Status:Checked
CL_Takeoff=Thrust Mode:Take Off
CL_Climb=Packs:On
CL_Climb=Engine Mode Selector:Normal
###
#
# Set V1, Vr and V2 for all possible flap settings (detents)
# Set the minimum and maximum airspeeds which are automatically
# mapped to the empty and max weights of the airplane
# Index is the flap detent, value is the KIAS
# Not all of the flap detents really make sense for takeoff
# but we can't anticipate all conditions so they should all
# be here.  You can have many [...]
V1Min[0]=120
V1Max[0]=170
V1Min[1]=120
V1Max[1]=170
V1Min[2]=120
V1Max[2]=170
V1Min[3]=131
V1Max[3]=168
V1Min[4]=131
V1Max[4]=161
VrMin[0]=128
VrMax[0]=182
VrMin[1]=128
VrMax[1]=182
VrMin[2]=128
VrMax[2]=182
VrMin[3]=131
VrMax[3]=179
VrMin[4]=131
VrMax[4]=172
V2Min[0]=136
V2Max[0]=190
V2Min[1]=136
V2Max[1]=190
V2Min[2]=136
V2Max[2]=190
V2Min[3]=150
V2Max[3]=189
V2Min[4]=147
V2Max[4]=181
# ------------------------------------------------
# Speed Climb (VVI and Speed)
# ------------------------------------------------
# VVI and speed are automatically set by CoPilot by Levels/Steps. (Note the
# [1] is AGL, the other are Feets). You can have many [...]
speedclimbaltbottom[0]=0
speedclimbaltup[0]=3000
speedclimbspeedvvi[0]=2500
speedclimbspeed[0]=220
speedclimbaltbottom[1]=1500
speedclimbaltup[1]=3000
speedclimbspeedvvi[1]=2500
speedclimbspeed[1]=250
speedclimbaltbottom[2]=3000
speedclimbaltup[2]=10000
speedclimbspeedvvi[2]=2200
speedclimbspeed[2]=250
speedclimbaltbottom[3]=10000
speedclimbaltup[3]=20000
speedclimbspeedvvi[3]=2200
speedclimbspeed[3]=330
speedclimbaltbottom[4]=20000
speedclimbaltup[4]=26000
speedclimbspeedvvi[4]=1800
speedclimbspeed[4]=330
speedclimbaltbottom[5]=26000
speedclimbaltup[5]=29000
speedclimbspeedvvi[5]=1500
speedclimbspeed[5]=330
speedclimbaltbottom[6]=29000
speedclimbaltup[6]=33000
speedclimbspeedvvi[6]=1500
speedclimbspeed[6]=305
speedclimbaltbottom[7]=33000
speedclimbaltup[7]=37000
speedclimbspeedvvi[7]=1000
speedclimbspeed[7]=278
speedclimbaltbottom[8]=37000
speedclimbaltup[8]=45000
speedclimbspeedvvi[8]=1000
speedclimbspeed[8]=255
# ------------------------------------------------
# Speed Descent (VVI and Speed)
# ------------------------------------------------
# VVI and speed are automatically set by CoPilot by Levels/Steps. (Note the
# [1] is AGL, the other are Feets). You can have many [...]
speeddescentaltbottom[0]=0
speeddescentaltup[0]=3000
speeddescentspeedvvi[0]=800
speeddescentspeed[0]=160
speeddescentaltbottom[1]=3000
speeddescentaltup[1]=5000
speeddescentspeedvvi[1]=2000
speeddescentspeed[1]=230
speeddescentaltbottom[2]=5000
speeddescentaltup[2]=10000
speeddescentspeedvvi[2]=1900
speeddescentspeed[2]=250
speeddescentaltbottom[3]=10000
speeddescentaltup[3]=37000
speeddescentspeedvvi[3]=2500
speeddescentspeed[3]=280
speeddescentaltbottom[3]=37000
speeddescentaltup[3]=45000
speeddescentspeedvvi[3]=2500
speeddescentspeed[3]=260
