DASSAULT FALCON 7X
REFERENCE INFORMATION
For standard procedures, see the Checklists tab.

Total Flight Simulator aircraft weight with full fuel | 63,600 lbs

NOTE: To adjust fuel load, on the Aircraft menu, click Fuel and Load.

VMO - Maximum Operating Speed | 350 KIAS
MMO - Maximum Operating Speed Mach | .90 Mach
d>
VLO - Maximum Gear Operating Speed | 200 KIAS
VLE - Maximum Landing Gear Extension Speed | 250 KIAS

Maximum Flap Placard Speeds

Flaps degrees | KIAS
10 | 250
20 | 200
40 | 150

V1 - Takeoff Decision Speed dry runway
Standard temperature, sea level pressure altitude

All conditions | 134 KIAS

VR - Rotation Speed dry runway
Standard temperature, sea level pressure altitude

All conditions | 135 KIAS

V2 - Minimum Climb Speed dry runway
Standard temperature, sea level pressure altitude

38200 lbs | 160 KIAS

VREF - Landing Approach Speed flaps 40, gear down
Standard temperature, sea level pressure altitude

38200 lbs | 110 KIAS

+++NOTAMS+++
Open the Panel_Docs folder for information on operating this aircraft.
Turn on Tool Tips
Panel Help available in the REF section of the Kneeboard
The Fuel Crossfeed Button must be in the On position for a balanced fuel burn.
Use Shift E to operate the Passenger Airstair
Important... If using AUTOSTART (CTRL E)...
Check to make sure the generators are switched to ON in the lower panel or VC
Use of +5 to +7º elevator trim is recommended for takeoff
For best frame rates...keep popup windows closed
Copyright © 2009 - Premier Aircraft Design