PREMIER AIRCRAFT DESIGN

BOMBARDIER DHC8-Q400

REFERENCE INFORMATION

For standard procedures see Checklist tab

Flight simulator aircraft max weight with full fuel 63,000 lbs

To adjust fuel load, on aircraft menu, click "Fuel & Load"

Max Operating Speed @ FL250 290 kts IAS

Minimum Control Speed 103 kts IAS

FLAPS

Maximum flaps extend speeds:

Flaps 5 190

Flaps 10 180

Flaps 15 170

Flaps 35 140

TAKE OFF DECISION SPEED:

Dry runway, standard temperature

Max weight 150 kts IAS

45,000 lbs 135 kts IAS

Vr Rotation Speed:

Max weight 148 kts IAS

45,000 lbs 120 kts IAS

V2 Take Off Safety Speed:

Max weight 148 kts IAS

45,000 lbs 142 kts IAS

Landing Approach Speed - Flaps 15 - Gear down:

45,000 lbs 140 kts IAS

FLIGHT SIMULATOR EYEPOINT ADJUSTMENTS:

Move eyepoint back

CTRL+ENTER

Move eyepoint down

CTRL+BACKSPACE

Move eyepoint Forward

CTRL+BACKSPACE

Move eyepoint left

CTRL+SHIFT+BACKSPACE

Move eyepoint right

CTRL+SHIFT+ENTER

Move eyepoint up

SHIFT+ENTER

Reset eyepoint

SPACE

---end ---