IRIS MIG-29 FULCRUM
REFERENCE INFORMATION

For more information in how to fly the aircraft, please refer to the Flight Handbook.

Total Flight Simulator aircraft weight with full fuel | 33,112 lbs

NOTE: To adjust fuel load, on the Aircraft menu, click Fuel and Load.

VMO - Maximum Operating Speed | 1,315 KM/H
MMO - Maximum Operating Speed Mach | 2.30 Mach
VLO - Maximum Gear Operating Speed | 380 KM/H
VLE - Maximum Landing Gear Extension Speed | 350 KM/H
Best Glide Speed | 160 KM/H

Maximum Flap Placard Speeds

Flaps degrees | KM/H
10 | 450
20 | 380
30 | 320
40 | 280

V1 - Takeoff Decision Speed dry runway
Standard temperature, sea level pressure altitude

All conditions | 100 KM/H

VR - Rotation Speed dry runway
Standard temperature, sea level pressure altitude

13,200 lbs | 135 KM/H
20,200 lbs | 140 KM/H

V2 - Minimum Climb Speed dry runway
Standard temperature, sea level pressure altitude

13,200 lbs | 130 KM/H
20,200 lbs | 140 KM/H

VREF - Landing Approach Speed flaps 40, gear down
Standard temperature, sea level pressure altitude

13,200 lbs | 130 KM/H
20,200 lbs | 135 KM/H

NOTE: For explanations of speeds used on this tab, see "V-speeds" in the Learning Center Glossary.