#Checklister by After
#for falcon 7x
Check list Falcon 7x
Bonjour et bienvenue a bord du 7x
procedure demarrage
batterie one on
batterie two on
avionics on
Check fuel valve open
select fuel tanks
Start apu
start apu generator
check inverter one on
check inverter two on
set cockpit light as you like
switch bleed command to apu
start engine left
switch generator left on
start engine center
switch generator center on
start engine right
switch generator right on
switch syncro n1 on
switch fadec on
switch hydraulic pump on
checkpressurization bleed altitude off
checkpressurization bleed all off
switch ice detect on
switch pilot heat on
switch copilot heat on
close door shift F1

check list before take off
switch bleed command to both
switch off apu generator
switch off apu
seatbelt on
no smoking on
switch on nav beacon strobelight
switch on taxi land light on if necessary
switch on TOT (take off trim) on
set flap to position one
release brake
put full throotle
plane should take off at around 160 kts depend on weight

checklist after take off
gear up
flap up
set desired altitude
set vvi to 2500
adjust throtle
set pressurization cabin to altitude 3000

check list before landing
set pressurization to altitude 0
set speed brake arm on
set auto brake to 2



