BOEING 717-200 PROCEDURES

____________________________________
BEFORE START CHECKLIST

[ ] Parking Brake -- SET
[ ] Transponder/TCAS -- ON
[ ] External Preflight -- COMPLETED
[ ] Logbooks/Checklists -- CHECKED
[ ] Electrical Panel -- SET
[ ] Battery Switch -- ON LOCKED
[ ] Fuel Tank Pumps/ X-FEED -- CHECKED OFF
[ ] Pitot Heat -- OFF
[ ] Engine Anti-Ice -- OFF
[ ] Stall and Max Speed Warnings -- CHECKED
[ ] Yaw Damper -- ON
[ ] Mach Trim -- NORMAL
[ ] Exterior Lights -- SET
[ ] NAV/FGS Panels -- CHECKED and SET
[ ] Altimeters/ Flight Instruments -- CHECKED and SET
[ ] Fuel Required -- ON BOARD
[ ] Gear Lights/Horn -- CHECKED
[ ] Stabilizer Trim -- CHECKED
[ ] Spoilers -- RETRACT
[ ] Throttles -- CHECKED/IDLE
[ ] Flaps -- UP/RETRACT
[ ] Radios/Trans/TCAS/ACARS -- CHECKED/SET
[ ] Stabilizer Trim Brake Switch -- NORMAL
[ ] Rudder/Aileron Trim -- ZERO
[ ] Autobrakes -- DISARM/OFF
[ ] Departure Briefing -- COMPLETE
[ ] Door Lights -- CHECKED
[ ] Anti-Collision Lights -- ON
[ ] Fuel Tank Pumps -- AS REQUIRED
[ ] Ignition -- ON

____________________________________
ENGINE START CHECKLIST

[ ] Ignition -- OFF
[ ] Generators -- CHECKED
[ ] Engine Instruments -- CHECKED
[ ] Pitot Heat -- ON
[ ] Engine Anti-Ice -- AS REQUIRED

____________________________________
AFTER START CHECKLIST

[ ] Engine Start Switches -- CHECK GEN
[ ] Pitot Heat -- ON
[ ] De-ice -- AS REQUIRED
[ ] Engine Start Levers -- CHECK IDLE
[ ] Lights -- AS REQUIRED
[ ] Autopilot -- SET and OFF
[ ] Instruments -- CHECKED
[ ] Autobrake Switch -- RTO (Rejected Takeoff)
[ ] Avionics Switch -- ON
[ ] Avionics -- SET
[ ] Altimeters -- CHECKED
[ ] Airspeed Bugs  -- CHECKED


____________________________________
TAXI CHECKLIST

[ ] Brakes -- RELEASE
[ ] Thrust Levers -- IDLE FOR TAXI
[ ] Flight Controls -- CHECK
[ ] Pitot Heat: ON


____________________________________
BEFORE TAKEOFF CHECKLIST

[ ] Flaps/Slats -- T/O
[ ] Engine Start Switches -- GEN
[ ] Flight Director -- ON
[ ] Autothrottle -- ARM
[ ] Transponder -- ON
[ ] Lights -- AS REQUIRED
[ ] Annunciator Panel/Warning Lights -- CHECKED
[ ] Takeoff Briefing -- COMPLETE
[ ] Brakes -- RELEASE
[ ] Engine Instruments -- MONITOR

____________________________________
AFTER TAKEOFF CHECKLIST

[ ] Landing Gear -- UP (WHEN POSITIVE CLIMB ESTABLISHED)
[ ] Ignition -- AS REQUIRED
[ ] Airspeed --MAINTAIN V2+20 KIAS
[ ] Autopilot -- ENGAGE AT 1,000' AGL
[ ] Flaps-- RETRACT 
[ ] Flaps-- UP AT 210 KIAS
    (press F6 until Up)
[ ] Autothrottle -- OFF
[ ] Airspeed -- 250 KIAS AT 3,000' AGL
[ ] Landing Gear Lever -- Verify OFF
[ ] Autobrakes/Spoilers -- OFF/DISARMED

____________________________________
CLIMB CHECKLIST

[ ] Landing Lights -- OFF ABOVE 10,000' MSL
[ ] Altimeter -- SET TO 29.92 CROSSING 18,000' MSL

____________________________________
CRUISE CHECKLIST

[ ] Thrust Levers-- AS DESIRED
[ ] Trim -- AS NECESSARY

____________________________________
DESCENT CHECKLIST

[ ] Autobrake Switch -- AS DESIRED
[ ] Airspeeds (VREF, VAPP) -- COMPUTED and SET
[ ] De-ice -- AS REQUIRED
[ ] Autopilot -- AS DESIRED
[ ] Thrust Levers -- AS DESIRED
[ ] Altimeter -- SET TO LOCAL SETTING CROSSING 18,000' MSL
[ ] Avionics -- SET
[ ] Airspeed -- <250 KIAS BELOW 10,000' MSL
[ ] Landing Lights -- ON BELOW 10,000' MSL
[ ] Approach Procedure -- REVIEW

____________________________________
APPROACH CHECKLIST

[ ] Airspeed -- AS DESIRED
[ ] Fuel Pumps/X-Feed -- AS REQUIRED/OFF
[ ] Thrust Levers -- AS DESIRED
[ ] Flaps -- AS DESIRED
[ ] Autopilot -- AS DESIRED
[ ] Autothrottle -- ARM
[ ] Aproach Briefing: COMPLETE
[ ] Altimeters -- CHECKED
[ ] NAV Set Up -- CHECKED

________________________________
LANDING CHECKLIST

[ ] Airspeed -- AS DESIRED
[ ] Ignition -- AS REQUIRED
[ ] Thrust Levers -- AS DESIRED
[ ] Speedbrake -- ARMED
[ ] Landing Gear -- DOWN AND CONFIRMED
[ ] Flaps -- AS DESIRED
[ ] Start Switches -- GEN
[ ] Autopilot -- AS DESIRED
[ ] Spoilers -- ARM

____________________________________
AFTER LANDING CHECKLIST

[ ] Flaps -- UP
[ ] Ignition -- OFF
[ ] Pitot Heat/Airfoil Anti-Ice -- OFF
[ ] Exterior Lights -- SET
[ ] Transponder/TCAS -- SET
[ ] Thrust Levers -- IDLE
[ ] Autopilot -- CHECK DISENGAGED
[ ] Autothrottle -- CHECK OFF
[ ] Spoilers -- RETRACT


____________________________________
SHUTDOWN CHECKLIST
[ ] Anti-Collision Lights -- OFF
[ ] Engine Anti-Ice -- OFF
[ ] AUX/Trans Hydraulic Pumps -- OFF
[ ] Parkingbrakes -- AS REQUIRED
[ ] Flight Director -- OFF

____________________________________
PARKING CHECKLIST

[ ] Parking Brake -- SET
[ ] Start Levers -- CUTOFF
[ ] De-ice -- OFF
[ ] Lights -- AS REQUIRED
[ ] Speedbrake Lever -- DOWN
[ ] Transponder -- AS REQUIRED

