A
750 version
x    y 
20   0	// comment: VVI needle offset center of rotation (right side)
-5   0	// comment: VVI autopilot bug offset (vertical linear path)
ENTER THE SAME VALUES IN THE FIRST AND SECOND LINES TO HAVE THE AUTOPILOT BUG MOVE ALONG AN ARC LIKE THE NEEDLE,
NOT A STRAIGHT VERTICAL TRACK, AS IT WILL IF YOU ENTER DIFFERENT VALUES ABOVE.
REMEMBER, THE CUSTOM LIMITS SCREEN IN PLANE-MAKER WILL SET ALL YOUR LIMIT ANGLES AND VALUES FOR THINGS
LIKE AIRSPEED, VERTICAL SPEED, ETC.