#GoodWay v2.3.0
#Fr Aug 20 11:31:02 CET 2004
cruise_speed=424
descent_rate=2500
descent_speed=270
plane_constructor=Boeing
xplane_certified=811
author=Morten Melhuus
cruise_altitude=41000
plane_type=B737-700
max_seats=140
plane_full_name=Boeing 737-700 Air Berlin
release_date=May 27 2005 1\:52\:26 PM
fuel_max_onboard=5311
climb_speed=270
plane_compagny=Air Berlin
release=beta27
fuel_max_consumption_hour=1099
author_web=http\://xplanefreeware.net/
maximum_range=2685
climb_rate=2200
###
# Added for CP
takeoff_flaps=3
takeoff_flaps_heavy=2
takeoff_flaps_heavy_threshold=155000
landing_flaps=6
###
# Optional equipment
HasRadarAltimeter=TRUE
# 0=none, 1=FMS/GPS, 2=Basic
AutoPilotType=1
###
# Text checklist items
# Separate the left hand and right hand text with a ':' and do
# not add extra space before/after ':'
CL_B4Start=Pressurization:Auto
CL_B4Start=Hydraulics:Set
CL_B4GateDeparture=Sliding Windows:Both Locked
CL_B4GateDeparture=Doors and slides:Green, Armed
CL_B4GateDeparture=Notify dispatch:CHECK
CL_B4Taxi=ECAM Status:Checked
CL_Takeoff=Thrust Mode:Take Off
CL_Climb=Packs:On
CL_Climb=Engine Mode Selector:Normal
###
#
# Set V1, Vr and V2 for all possible flap settings (detents)
# Set the minimum and maximum airspeeds which are automatically
# mapped to the empty and max weights of the airplane
# Index is the flap detent, value is the KIAS
# Not all of the flap detents really make sense for takeoff
# but we can't anticipate all conditions so they should all
# be here.  You can have many [...]
V1Min[0]=122
V1Max[0]=160
V1Min[1]=99
V1Max[1]=143
V1Min[2]=96
V1Max[2]=140
V1Min[3]=93
V1Max[3]=132
VrMin[0]=127
VrMax[0]=169
VrMin[1]=101
VrMax[1]=146
VrMin[2]=98
VrMax[2]=142
VrMin[3]=95
VrMax[3]=132
V2Min[0]=114
V2Max[0]=152
V2Min[1]=114
V2Max[1]=152
V2Min[2]=111
V2Max[2]=148
V2Min[3]=107
V2Max[3]=138

# ------------------------------------------------
# Speed Climb (VVI and Speed)
# ------------------------------------------------
# VVI and speed are automatically set by CoPilot by Levels/Steps. (Note the
# [1] is AGL, the other are Feets). You can have many [...]
speedclimbaltbottom[0]=0
speedclimbaltup[0]=1500
speedclimbspeedvvi[0]=2500
speedclimbspeed[0]=220
speedclimbaltbottom[1]=1500
speedclimbaltup[1]=3000
speedclimbspeedvvi[1]=2500
speedclimbspeed[1]=250
speedclimbaltbottom[2]=3000
speedclimbaltup[2]=10000
speedclimbspeedvvi[2]=2200
speedclimbspeed[2]=250
speedclimbaltbottom[3]=10000
speedclimbaltup[3]=20000
speedclimbspeedvvi[3]=2200
speedclimbspeed[3]=280
speedclimbaltbottom[4]=20000
speedclimbaltup[4]=26000
speedclimbspeedvvi[4]=1800
speedclimbspeed[4]=290
speedclimbaltbottom[5]=26000
speedclimbaltup[5]=41000
speedclimbspeedvvi[5]=1200
speedclimbspeed[5]=300
# ------------------------------------------------
# Speed Descent (VVI and Speed)
# ------------------------------------------------
# VVI and speed are automatically set by CoPilot by Levels/Steps. (Note the
# [1] is AGL, the other are Feets). You can have many [...]
speeddescentaltbottom[0]=0
speeddescentaltup[0]=3000
speeddescentspeedvvi[0]=800
speeddescentspeed[0]=133
speeddescentaltbottom[1]=3000
speeddescentaltup[1]=5000
speeddescentspeedvvi[1]=2000
speeddescentspeed[1]=230
speeddescentaltbottom[2]=5000
speeddescentaltup[2]=10000
speeddescentspeedvvi[2]=1900
speeddescentspeed[2]=250
speeddescentaltbottom[3]=10000
speeddescentaltup[3]=41000
speeddescentspeedvvi[3]=2500
speeddescentspeed[3]=290
