DSB DESIGN HAWK REFERENCE INFORMATION

For standard procedures, see the Checklists tab.

Total Flight Simulator aircraft weight with full fuel
           12,566 lbs

NOTE: To adjust fuel load, on the Aircraft menu, click Fuel.

VMO - Maximum Operating Speed (airspeed)
           560 KIAS (primary display)

MMO - Maximum Operating Speed (Mach)
	0.92 Mach (autopilot disengaged)

VA  -  Maneuvering Speed
          11,100 lbs.
          250 KIAS (sea level)

VLO - Maximum Gear Operating Speed
          260 KIAS

VLE - Maximum Landing Gear Extension Speed
          300 KIAS

VFE - Maximum Flaps Extended Speed
          280 KIAS

V1 - Takeoff Decision Speed (dry runway; standard temperature)
	120 KIAS

VR - Rotation Speed (dry runway; standard temperature)
        Sea Level
        90 KIAS (27,500 lbs)

V2 - Takeoff Safety Speed (dry runway, standard temperature)
        Sea Level
        170 KIAS

VREF - Landing Approach Speed (full flaps; gear down)
	130 KIAS (10,500 lbs)

Landing touchdown speed
	100 KIAS

Best Glide Speed
	170 KIAS (gear and flaps up; both engines inoperative)

Stall speed, clean, full fuel
	80 KIAS

Stall speed, gear down, full flaps
	70 KIAS	

NOTE:  For explanations of speeds used on this tab, see "V-speeds" in the Glossary section of Help.