MOONEY BRAVO
REFERENCE INFORMATION
For detailed instructions on how to fly this aircraft, see the Aircraft Information
articles in the Learning Center. For standard procedures, see the Checklists tab.

Total Flight Simulator aircraft weight with full fuel | 3,326 lbs

NOTE: To adjust fuel load, on the Aircraft menu, click Fuel and Load.

VA - Maneuvering Speed (3,368 lbs) | 127 KIAS
VA - Maneuvering Speed (3,200 lbs) | 123 KIAS
VA - Maneuvering Speed (2,900 lbs) | 117 KIAS
VNO - Max Structural Cruising Speed | 174 KIAS
VNE - Never Exceed Speed | 195 KIAS
VLE - Maximum Gear Extension Speed | 165 KIAS
VS - Stalling Speed (max weight, flaps up) | 66 KIAS
VSO - Stalling Speed in Landing Configuration | 59 KIAS
VX - Best Angle-of-Climb Speed (sea level) | 85 KIAS
VY - Best Rate-of-Climb Speed (sea level) | 105 KIAS
Best Glide Speed (3,368 lbs) | 93.5 KIAS
Best Glide Speed (3,200 lbs) | 89 KIAS
Best Glide Speed (2,900 lbs) | 84.5 KIAS
Best Glide Speed (2,600 lbs) | 80 KIAS

Maximum Flap Placard Speeds

Flaps degrees | KIAS
Full flaps | 110

NOTE: For explanations of speeds used on this tab, see "V-speeds" in the Learning Center Glossary.