BOEING B-575 PROCEDURES

For detailed instructions on how to fly this aircraft, see the Aircraft Information section of Help. For suggested speeds, see the Reference tab.

____________________________________
BEFORE STARTING ENGINES

[ ] Gear -- CHECK DOWN
[ ] BATT Switch -- ON
[ ] L and R GEN Switches -- OFF
[ ] Flight Controls -- CHECK
[ ] Engine Instruments -- CHECK
[ ] Fuel Quantity -- CHECK
[ ] Aircraft Lighting -- OFF
[ ] Parking Brake -- SET
     (or press CTRL + PERIOD key)
[ ] Trim -- set to 3 notches up.
     (Num Lock off. Num Pad 1/Num Pad 7)
[ ] Altimeters -- SET
[ ] Takeoff Data (V1, VR, V2) -- COMPUTED AND SPEEDS SET
     (see the Reference tab of the kneeboard)
[ ] Avionics Master Switch -- ON
[ ] Avionics -- SET FOR DEPARTURE

____________________________________
STARTING ENGINES

Press CTRL+E to initiate engine autostart sequence, or:
 
[ ] Switch on Beacons.
[ ] PARKING BRAKE -- SET
     (or press CTRL + PERIOD key)
[ ] Thrust Levers -- IDLE
     (or press F2 or F3 as necessary)
[ ] Fuel Flow -- ON
	CTRL+SHIFT+F4.
[ ] L Start Switch -- ON
	hold until engine starts.
[ ] L FF (Fuel Flow) -- CHECK
[ ] L N1 increasing as L N2 increases -- CHECK
[ ] L ITT -- CHECK
[ ] L Oil Pressure -- CHECK
[ ] L Engine Instruments -- CHECK NORMAL
[ ] R Start Switch -- ON
	hold until engine starts.
[ ] R FF (Fuel Flow) -- CHECK
[ ] R N1 increasing as L N2 increases -- CHECK
[ ] R ITT -- CHECK
[ ] R Oil Pressure -- CHECK
[ ] R Engine Instruments -- CHECK NORMAL
[ ] L and R GEN Switches -- ON
[ ] OR use AUTO for full Auto start.

____________________________________
BEFORE TAXI

[ ] Spoiler Lever -- ARM
     (or SHIFT + / (FORWARD SLASH key))
[ ] Flaps -- SET 1 notch
     (press F6 or F7)
[ ] Flight Controls -- CHECK
[ ] Aircraft Lighting -- ON AS REQUIRED
[ ] Brakes -- RELEASE
     (or press PERIOD key)

____________________________________
TAXI AND BEFORE TAKEOFF

[ ] Brakes -- CHECK
     (or press PERIOD key)
[ ] Flight Instruments -- CHECKED
[ ] Engine Instruments -- CHECK
[ ] Takeoff Data (V1, VR, V2) -- CHECK
     (see the Reference tab of the kneeboard)
[ ] Nav Equipment -- CHECK
[ ] Flaps -- SET 1 notch
     (or press F6 or F7)
[ ] Trim -- SET FOR TAKEOFF
     (Num Lock off. Num Pad 1/Num Pad 7)

____________________________________
RUNWAY LINEUP

[ ] Lights -- ON

____________________________________
TAKEOFF

[ ] Thrust Lever -- Full
     (or press F3 until Full)
[ ] Brakes -- RELEASE
     (or press PERIOD key)
[ ] VR -- ROTATE at 115kts

____________________________________
AFTER TAKEOFF

[ ] Gear -- UP at 100 ft agl.
[ ] Flaps -- UP at 200 kts.
[ ] SPOILER LEVER -- RET
	(or SHIFT + / (FORWARD SLASH key until retracted)

____________________________________
CLIMB

[ ] Engage autopilot.
[ ] Altimeters -- RESET TO 29.92 CROSSING 18,000 FEET
	or Auto set

____________________________________
DESCENT

[ ] Altimeters -- RESET TO LOCAL CROSSING 18,000 FEET
[ ] Fuel Quantities and Balance -- CHECK

____________________________________
APPROACH

[ ] Landing Data (VREF, VAPP) -- COMPUTED AND SPEEDS SET
     (see the Reference tab of the kneeboard)
[ ] Avionics and Radios -- SET
[ ] Flaps -- Full
     (or F6 or F7 as necessary)
[ ] Spoiler Lever -- ARM
     (or SHIFT + / (FORWARD SLASH key))

____________________________________
BEFORE LANDING

[ ] Autobrakes to 3 for a 5000 ft & above runway, 
	to maximum for a 2500 ft grass one.
[ ] Airbrakes to autodeploy. 
[ ] Gear -- DN (Check for 3 green lights)
	(or G)
	LDG (as reqd)-TAXI Light

____________________________________
LANDING
[ ] POWER to IDLE
[ ] Thrust reverser (F2)
[ ] Brakes -- AS REQUIRED
     (or PERIOD key)
[ ] Spoilers -- VERIFY EXTENDED

____________________________________
AFTER LANDING/CLEARING RUNWAY

[ ] Lights -- AS DESIRED
[ ] Spoiler Lever -- RET
     (press SHIFT + / (FORWARD SLASH key) until retracted)
[ ] Flaps -- UP
     (press F6 until Up)
[ ] Thrust Lever -- CUTOFF
     (press F2 until Cutoff)

____________________________________
SHUTDOWN

[ ] Parking Brake -- SET
	(or CTRL + PERIOD key)
[ ] Thrust Levers -- IDLE
	(or F2 until Idle)
[ ] Fuel Flow -- OFF
	(or CTRL+SHIFT+F1)
[ ] Lights -- OFF
[ ] L and R GEN Switches -- OFF
[ ] BATT Switch -- OFF
