Lider Designs Gulfstream GV 
for Flight Simulator 2004.


Copyrights LiderDesigns.


Visit www.liderdesigns.com for more information os the projects.


Peter Brun
Caracas / Venezuela
peter@liderdesigns.com

Model By: Peter Brun

Panel By: Default LearJet

Textures By: Peter Brun

Freeware version By LiderDesigns

Performance 

Maximun Range 5,800nm / 10,742Km
(8 passengers and 4crew and NBAA IFR Fuel reserves)

Long-RangeCruise Speed Mach 0.80 / 459 Ktas / 850 Km/h

Normal Cruise Speed Mach 0.75 / 430 Ktas / 796 Km/h

Mmo (Maximun Operating Mach Number) Mach 0.885

TakeOff Distance 5,150 ft / 1,570 m

Landing Distance 2,770 ft / 844 m

Initial Cruise Altitude 431,000 ft / 13,106 m

Maximun Cruise Altitude 51,000 ft / 15,545 m


Weights

Maximun Takeoff Weight 85,100 lb / 38,601 kg

Maximun Landing Weight 75,300 lb / 34,156 kg

Maximun Zero Fuel Weight 54,500 lb / 24,721 kg

Basic Operating Weight 47,800 lb / 21,682 kg

Maximun Payload 6,700 lb / 3,039 kg

Payload with Maximun Fuel 2,500 lb / 1,134 kg

Maximun Fuel Weight 35,200 lb / 15,966 kg


Design Standards

Engines (2) Rolls-Royce BR710

Rated Takeoff Thrust (each) 15,385 lb /68.4 kN

Passengers: Typical Outfitting 14 - 18


Interior

Cabin Length 50ft 1 in / 15.3 m

Cabin Height 6 ft 2in / 1.88 m

Cabin Width 7ft 4in / 2.24 m

Cabin Volume 1,669 cu ft./ 47.3 cu m

Baggage Compartment Volume 226 cu ft / 6.4 cu m


Exterior

Lenght 96ft 5in / 29.4 m

Height 25ft 10in / 7.9 m

Wingspan 93ft 6in / 28.5 m


