Reference Data for De Havilland Otter NG by Stratojet
VMO - Max. authorized speed: | 300 KIAS
VLO - Max. speed for flaps | 225 KIAS
VLE - Max. speed for gear down | 225 KIAS
Cruising speed: | 220 KIAS @ 10.000 ft
Max. altitude: | 20.000ft
Range: ~ 3.500 km @ cruising speed and altitude
Take-off speed: ~ 90 KIAS with flaps 10
Min. Landing speed: ~ 70 KIAS with flaps 40
Recommended Landing speed: ~ 90 KIAS with flaps 30
Technical Data: |
Length: | 15,2 m
Height: | 6,2 m (with gear down)
Wing span: | 17,8 m
Empty weight: | 4.800 pounds
Max gross weight: | 11.000 pounds
Fuel capacity: | 2x 225 gallons
Engine: | 1x Turboprop
| General Electric CT7-9D
Horsepower: | 1.940 shp
Torque: | 5.500 ft-lbs