GRUMMAN G21-A GOOSE
REFERENCE INFORMATION
For detailed instructions on how to fly this aircraft, see the Aircraft Information
articles in the Learning Center. For standard procedures, see the Checklists tab.

Total Flight Simulator aircraft weight with full fuel | 9200 lbs

NOTE: To adjust fuel load, on the Aircraft menu, click Fuel and Load.

VMC - Minimum Control Speed | 94 MPH
VNE - Never Exceed Speed | 225 MPH
VFE - Flaps Extension Speed | Not Required
VS - Stalling Speed (max weight, flaps up) | 70 MPH
VSO - Stalling Speed in Landing Configuration | 60 MPH
VSE - Best Angle-of-Climb Speed (sea level) | 108 MPH

NOTE: For explanations of speeds used on this tab, see "V-speeds" in the Learning Center Glossary.