AN158
REFERENCE INFORMATION
For detailed instructions on how to fly this aircraft, see the Aircraft Information
articles in the Learning Center. For standard procedures, see the Checklists tab.

Total Flight Simulator aircraft weight with full fuel | 96,672 lbs

NOTE: To adjust fuel load, on the Aircraft menu, click Fuel and Load.

VMO - Maximum Operating Speed | 310 KIAS
MMO - Maximum Operating Speed Mach | .80 Mach
Turbulent Air Penetration Speed | 280 KIAS/.73 Mach
VLO - Maximum Gear Operating Speed | 200 KIAS
VLE - Maximum Landing Gear Extension Speed | 216 KIAS

Maximum Flap Operation Speeds

Flaps degrees | KIAS
0 | 216
10 | 216
20 | 210
40 | 173