Beech 18Checklist

TAKEOFF AND CLIMB (at sea level)
[ ] Brakes | RELEASE
[ ] Mixtures | RICH AS NEEDED
[ ] Throttles | FULL 1 MINUTE MAX
[ ] Propellers | 2300RPM
[ ] ROTATE @ 105 KTS
[ ] Landing Gear | RETRACT (positive climb established)
[ ] Airspeed | 115-120 KIAS
CLIMB (once obstacles cleared, or 300 AGL)
[ ] Throttles | 32 MAP
[ ] Propellers | 2200 RPM
[ ] Airspeed | 105 KIAS
CLIMB (approx. 500 AGL)
[ ] Flaps | UP
[ ] Throttles | 32 MAP
[ ] Propellers | 2200 RPM
[ ] Mixture | LEAN AS REQD
[ ] Trim | SET FOR CLIMB
[ ] Temperature/Pressures | CHECK
[ ] Fuel Selector | WING MAINS
[ ] Boost Pumps | OFF (one at a time)
[ ] Landing Lights | OFF / RETRACTED
[ ] Airspeed | 105 KIAS

BACK NEXT

NOTE: This aircraft's real-world checklists have been modified for use with Flight Simulator.