Beech 18 Checklist

APPROACH
[ ] Airspeed | SLOW FROM 180 Kts to 139
[ ] Mixtures | RICH
[ ] Throttles | AS REQ’D
[ ] Propellers | FULL FORWARD
[ ] Fuel Selector | FRONT
[ ] Boost Pumps | ON
[ ] Cowl Flaps | OPEN HALFWAY
[ ] Carb Heat | AS REQUIRED
[ ] Flaps | ONE NOTCH
[ ] Landing Gear | DOWN @ 139 Kts
[ ] Landing Lights | ON
FINAL
[ ] Flaps/Airspeed | 15*/105 Kts
[ ] Flaps | 25*/95 Kts
[ ] Flaps | 45*/85 Kts (Under Power)
[ ] Throttles | AS REQ’D
[ ] Landing Gear | CHECK
Touch down at 80 KIAS, Close Throttles

BACK NEXT

NOTE: This aircraft's real-world checklists have been modified for use with Flight Simulator.