Beech 18 Checklist

CRUISE
[ ] Throttles | 30” Hg MAP
[ ] Propellers | 2000 RPM
[ ] Mixtures | SET AS REQ’D
[ ] Cowl Flaps | CLOSED (AS REQ”D)
[ ] Fuel Valves | WING MAINS
Econo Cruise about 190 KIAS
DESCENT
[ ] Throttles | 28”-21” Hg MAP
[ ] Propellers | 2000 RPM
[ ] Mixtures | SET AS REQ’D
[ ] Hydraulic Pressure | CHECK
[ ] Airspeed | BELOW Vno

BACK NEXT

NOTE: This aircraft's real-world checklists have been modified for use with Flight Simulator.