Beech 18 Checklist

ENGINE STARTING
Press CTRL+E to initiate engine autostart sequence, or:
MANUAL ENGINE STARTING
Start right engine first
[ ] Mixture | FULL RICH
[ ] Throttle | CRACKED
[ ] Propeller Control | FULL FORWARD
[ ] Battery Switch | ON
[ ] Fuel Boost Pump | ON (right engine)
[ ] Magnetos | BOTH
[ ] Start Master Battery Switch | ON
[ ] Starter Selector | RIGHT
[ ] Primer | AS REQUIRED
[ ] Starter Switch | ENGAGE hold until engine starts
[ ] Oil Pressure | CHECK
[ ] Fuel Pressure | CHECK
[ ] Fuel Boost Pump | OFF
[ ] Oil Pressure | CHECK
[ ] Fuel Pressure | CHECK
[ ] Vacuum Pressure | CHECK
[ ] Hydraulic Pressure | CHECK
REPEAT FOR LEFT ENGINE

BACK NEXT

NOTE: This aircraft's real-world checklists have been modified for use with Flight Simulator.