Beech 18 Checklist

ENGINE RUN-UP
[ ] Parking Brake | SET
[ ] Temps & Press | CHECK
[ ] Mixtures | BEST IDLE
[ ] Throttles | 1500 RPM
[ ] Props | EXERCISE
[ ] Feathering | CHECK(un-feather after 200 rpm drop)
[ ] Generators | CHECK
[ ] Heading Indicators | SET
[ ] Vacuum Press | CHECK
[ ] Pitot Heat | CHECK
[ ] Magnetos | CHECK <100 rpm drop on each; <40 rpm drop between
[ ] Throttles | 1000 RPM

BACK NEXT

NOTE: This aircraft's real-world checklists have been modified for use with Flight Simulator.